Příloha č. 3 ZD

**Technical parameters for upgrade of the detection system (2 CCD detectors with electronics)**

Frequency: 1 kHz

Number of pixels: 2048

Pixel width: 14 m

Pixel height: 1 mm

Spectral range: 200 - 1100 nm

ADC card: at least 16 bit

Input port: compatible with the exit port of monochromator Solar TII